Bullnose Garage – STL Files
https://bullnosegarage.com

FILE NAME:
BNG_Window_Crank_Knob

DESIGNER:
Ed Zenisek
Bullnose Garage

DESCRIPTION:
This is a snap-fit replacement knob for Bullnose Ford window cranks. The original factory knob was not designed to be serviceable, and this part follows the same approach. Print the two halves in ASA, align them, and snap them together—no glue, no hardware, and no inserts required. Once assembled, the knob rotates freely and installs just like the original.

This part is intended to snap together permanently. If removal or disassembly is required, simply print a new set.

VEHICLE FITMENT:
Bullnose Trucks and Broncos.  May fit other vehicles, but untested.

RECOMMENDED MATERIAL:
ASA

PRINT NOTES:
• Line Height: .12-.16
• Walls / perimeters: 3
• Other notes (if needed): Gyroid infill

HARDWARE / ASSEMBLY:
None

INSTALL NOTES:
Drill out original knob from Ford assembly and snap into place.  Non-removable.

DISCLAIMERS:
• Designed and tested on my own vehicle.
• Measure and verify fitment before final installation.
• Automotive environments involve heat, vibration, and UV exposure.

LICENSE:
See LICENSE.txt included with this download.